inorganic_stone_soil

Uristocrat: Soil density data from:
http://www.pedosphere.com/resources/bulkdensity/worktable_us.cfm
 
In spite of the weird URL, the site is normal.
 
DF is based on the texture triangle, which you can see here:
http://www.pedosphere.com/resources/bulkdensity/triangle_us.cfm
 
All of these are actually mixes of sand, silt & clay.  Loam is a
roughly equal mix of all three.  So I'll give the percentages of
each that I used to find the density.  For example, SCS = 20/60/20
means that a soil was assumed to contain 20% sand, 60% clay & 20%
silt.  The numbers will always be in the order sand/clay/silt.

[OBJECT:INORGANIC]

[INORGANIC:CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:clay][DISPLAY_COLOR:4:6:0][TILE:178]
[SOIL]
[SOLID_DENSITY:1210] SCS = 20/60/20
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]
[STATE_COLOR:ALL_SOLID:BRASS]

[INORGANIC:SILTY_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:silty clay][DISPLAY_COLOR:4:7:0][TILE:178]
[SOIL]
[SOLID_DENSITY:1210] SCS = 5/50/45
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]
[STATE_COLOR:ALL_SOLID:DARK_TAN]

[INORGANIC:SANDY_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:sandy clay][DISPLAY_COLOR:4:6:0][TILE:177]
[SOIL]
[SOLID_DENSITY:1330] SCS = 55/40/5
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]
[STATE_COLOR:ALL_SOLID:PEARL]

[INORGANIC:CLAY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:clay loam][DISPLAY_COLOR:4:7:0][TILE:177]
[SOIL]
[SOLID_DENSITY:1320] SCS = 33/34/33
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_EARTHENWARE]
[STATE_COLOR:ALL_SOLID:ECRU]

[INORGANIC:SANDY_CLAY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:sandy clay loam][DISPLAY_COLOR:4:6:0][TILE:176]
[SOIL][AQUIFER]
[SOLID_DENSITY:1410] SCS = 60/25/15
[STATE_COLOR:ALL_SOLID:FLAX]

[INORGANIC:SILTY_CLAY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:silty clay loam][DISPLAY_COLOR:4:7:0][TILE:176]
[SOIL][AQUIFER]
[SOLID_DENSITY:1290] SCS = 10/30/60
[STATE_COLOR:ALL_SOLID:GOLD]

[INORGANIC:LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:loam][DISPLAY_COLOR:6:7:0][TILE:176]
[SOIL][AQUIFER]
[SOLID_DENSITY:1410] SCS = 40/20/40
[STATE_COLOR:ALL_SOLID:SILVER]

[INORGANIC:SANDY_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:sandy loam][DISPLAY_COLOR:6:6:1][TILE:176]
[SOIL][AQUIFER]
[SOLID_DENSITY:1560] SCS = 65/10/25
[STATE_COLOR:ALL_SOLID:BUFF]

[INORGANIC:SILT_LOAM]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:silt loam][DISPLAY_COLOR:6:7:0][TILE:177]
[SOIL][AQUIFER]
[SOLID_DENSITY:1410] SCS = 20/15/65
[STATE_COLOR:ALL_SOLID:BEIGE]

[INORGANIC:LOAMY_SAND]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:loamy sand][DISPLAY_COLOR:6:6:1][TILE:177]
[SOIL][AQUIFER]
[SOLID_DENSITY:1690] SCS = 80/5/15
[STATE_COLOR:ALL_SOLID:PEARL]

[INORGANIC:SILT]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:silt][DISPLAY_COLOR:6:7:0][TILE:178]
[SOIL][AQUIFER]
[SOLID_DENSITY:1450] SCS = 10/10/80
[STATE_COLOR:ALL_SOLID:ECRU]

[INORGANIC:SAND_TAN]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:sand][DISPLAY_COLOR:6:4:1][TILE:176]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5
[STATE_COLOR:ALL_SOLID:TAN]

[INORGANIC:SAND_YELLOW]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:yellow sand][DISPLAY_COLOR:6:6:1][TILE:178]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5
[STATE_COLOR:ALL_SOLID:YELLOW]

[INORGANIC:SAND_WHITE]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:white sand][DISPLAY_COLOR:7:6:1][TILE:178]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5
[STATE_COLOR:ALL_SOLID:IVORY]

[INORGANIC:SAND_BLACK]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:black sand][DISPLAY_COLOR:0:6:1][TILE:178]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5
[STATE_COLOR:ALL_SOLID:TAUPE_DARK]

[INORGANIC:SAND_RED]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:red sand][DISPLAY_COLOR:4:4:1][TILE:176]
[SOIL][AQUIFER][SOIL_SAND]
[SOLID_DENSITY:1710] SCS = 90/5/5
[STATE_COLOR:ALL_SOLID:VERMILION]

[INORGANIC:PEAT]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:peat][DISPLAY_COLOR:0:6:1][TILE:176]
[SOIL][AQUIFER]
[SOLID_DENSITY:850]  Peat was much too high.  This assumes it has some water in it.
[STATE_COLOR:ALL_SOLID:MAROON]

[INORGANIC:PELAGIC_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:pelagic clay][DISPLAY_COLOR:4:6:0][TILE:176]
[SOIL_OCEAN][AQUIFER]
[SOLID_DENSITY:2200]
[STATE_COLOR:ALL_SOLID:CHARCOAL]
Undersea soil densities from "Geotechnical Properties of Deep Continental Margin Soils"
http://www.informaworld.com/index/907178093.pdf

Undersea soils are fairly dense, being compacted.

[INORGANIC:CALCAREOUS_OOZE]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:calcareous ooze][DISPLAY_COLOR:4:7:0][TILE:177]
[SOIL_OCEAN][AQUIFER]
[SOLID_DENSITY:2690]
[STATE_COLOR:ALL_SOLID:TAUPE_PURPLE]

[INORGANIC:SILICEOUS_OOZE]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:siliceous ooze][DISPLAY_COLOR:4:7:0][TILE:177]
[SOIL_OCEAN][AQUIFER]
[SOLID_DENSITY:2460]
[STATE_COLOR:ALL_SOLID:MIDNIGHT_BLUE]

[INORGANIC:FIRE_CLAY]
[USE_MATERIAL_TEMPLATE:SOIL_TEMPLATE]
[STATE_NAME_ADJ:ALL_SOLID:fire clay][DISPLAY_COLOR:4:6:0][TILE:178]
[SOIL]
[SOLID_DENSITY:2300]
[MATERIAL_REACTION_PRODUCT:FIRED_MAT:INORGANIC:CERAMIC_STONEWARE]
[STATE_COLOR:ALL_SOLID:RUST]